==============================================================================
  Schroff PXIe System Manager for Windows                   DATE: 24-05-2024
==============================================================================

DISCLAIMER OF WARRANTY. THE SOFTWARE (INCLUDING ANY ACCOMPANYING
WRITTEN MATERIALS OR FILES) ARE PROVIDED “AS IS” AND “AS AVAILABLE”
WITHOUT WARRANTY, EXPRESS OR IMPLIED, OF ANY KIND, INCLUDING WITHOUT
LIMITATION, WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A
PARTICULAR PURPOSE (EVEN IF nVent HAS BEEN ADVISED OF SUCH PURPOSE). 
NO ORAL OR WRITTEN INFORMATION OR ADVICE GIVEN BY nVent OR ITS DEALERS, 
DISTRIBUTORS, OR AGENTS, SHALL CREATE SUCH A WARRANTY. nVent
DOES NOT WARRANT THAT THE FUNCTIONS CONTAINED IN THE SOFTWARE WILL
MEET YOUR REQUIREMENTS, OR THAT THE OPERATION OF THE SOFTWARE WILL
BE UNINTERRUPTED OR ERROR-FREE, OR THAT THE SOFTWARE IS VIRUS-FREE,
OR THAT PROGRAM DEFECTS WILL BE CORRECTED.


Overview:
---------

With the "PXIe System Manager" software, PXIe systems can be monitored and 
controlled.The software is compatible with Schroff PXIe systems in connection 
with PXIe Embedded Controllers from Schroff.


INSTALLATION:
-------------

Before the PXIe System Manager can be run, please execute "PXIe System Setup"


USAGE:
------

To start the PXIe System Manager, the PXIe_System_Manager.exe must be executed.



CHANGES LOG:
------------
v2.3.1.4
- Current Windows builds lock install application through WMI interface. Added workaround for Windows Versions >= 11 24H2 

v2.3.1.3
- Added custom chassis 14393-007
- Patched 14579-032 EDF data

v2.3.1.1
- performce CPU check only when trying to install CGOS API 

v2.3.1.0
- includes support for Windows 11 version 24H2

v2.3.04
- fixed 64 Bit System Module DLL extraction

v2.3.03
- added Schroff Resource Manager and set it to inactive
- updated Schroff System Manager to Version 2.1.0
- added System Resources for 14579032
- updated Health check tool to Version 2.0
- added Chassis Management API (pxieChMgt.dll)
- added 64 Bit libraries for pxieChMgt.dll and System Module and Trigger Manager

v2.2.16
- fix for 21 Slot daisy chain

v2.2.14 (28-08-2024)
- fixed for 14579-044

v2.2.13 (24-05-2024)
- fixed ID for 14395-066

v2.2.12 (24-05-2024)
- Multi Chassis with daisy chaining capable
- Added Custom Chassis 14395-070, 14395-066

v2.2.10 (23-02-2024)
- Added variable paths into installing for better precheck
- Auto-Detect of System Controller in Health Check Tooling
- minor Bugfixing

v2.2.9 (09-02-2024)
- System Module Driver fixed in term of invalid memory access
- Initial Setup sets System Module Driver version in registry
- Health Check tool updated with new Chassis models (42-926-001, 42-925-001, 42-927-101) to version v1.1

v2.2.8 (19-01-2024)
- System Module Driver returns arrays of submodul, controller type and serial nummber according PXI-6 v1.4

v2.2.7 (09-01-2024)
- System Module 21265-170 added 
- Chassis Models 14396-063 and 42-927-101 added
- Health Check Tool updated with new System Modules and Chassis

v2.2.6 (12-12-2023)
- Chassis models 24394-125, 24394-126 added
- internal changes, product care in appearance and sub revision

v2.2.5 (12-09-2023)
- Chassis Models 42-927-101, 89624024, 90607093, 90582678, 14394-002 added 

SUPPORTED DEVICES in v2.3.03:
------------------
14579-030
14579-040
14579-032
14579-042
14579-033
14579-034
14579-043
14579-044
14396-035
14396-029
14396-023/42-924-001
14396-018/42-926-001
14396-018A1001/42-926-001
14399-151
24396-560
24397-535
24396-586
14396-030
14396-042/14396035
24395-252
14396-051/42-925-001
14396-051A1001/42-925-001
24396-075
24395-447
14395-056
24394-042
14395-052
14394-002
14394-007
24394-125
14396-063/42-927-101
24394-126
14395-063
14395-066
14395-070
14395-069
14395-073
14395-074
21990-817
21990-819
21990-823
21990-825
90582678
90607093
90624024
90537049
90643586
23297432
21265120
21265124
21265170

